AMENDMENT 2

* All areas can use riser rated cable as no plenum returns are above grid
* All WAP's will be Category 6A cable see attached updated specification for proper part numbers
* All portables will be copper terminated to the 1st closest portable IDF and removal of the fiber terminating to the second IDF portable will take place.
* Copper terminations in all classrooms will be a total of 8, removal of extra existing drops in the portables will not have replacement cable.  i.e. extra lab drops will be eliminated from replacement.
* Start date will be determined after the award date between Richland School and the awarded contractor.

**End of Amendment 2**